SERVICE MANUAL UPDATE-REVISED THROTTLE BODY FUEL RAIL TORQUE. Chevrolet Beretta 1987

For 1990-2009 cars

# SERVICE MANUAL UPDATE-REVISED THROTTLE BODY FUEL RAIL TORQUE

#### Model and Year: 1987-89 CELEBRITY, CAVALIER, CORSICA, BERETTA WITH 2.8L (VIN CODE W) ENGINE

The throttle body attaching bolt torque and fuel rail attaching bolt torque specifications, Section 6E3-C2 are incorrect in some service manuals. The correct torque specifications are:

Throttle body to plenum 25 N.m (18 lb. ft.) attaching bolts

Fuel Rail to intake 10 N.m (88 lb. in.) manifold attaching bolts

Intake plenum attaching 21 N.m (16 lb. ft.) bolts

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.