FRT. DOOR LOCK ROD RATTLES (NEW ANTI-RATTLE CLIPS). Chevrolet Beretta 1989

For 1990-2009 cars

# FRT. DOOR LOCK ROD RATTLES (NEW ANTI-RATTLE CLIPS)

#### VEHICLES AFFECTED: 1988-89 L AND W CARS

Customer comments of rattles in the door on 1988-89 L and/or W cars may be the result of loose lock rods in the anti-rattle clips. To correct this condition revised anti-rattle clips should be installed. (two anti-rattle clips on coupes, three anti-rattle clips on sedan front per door)

#### Parts Required:

Single anti-rattle clip, P/N 16608794 - one required per front door for coupe and sedan

Double anti-rattle clip, P/N 16609594 - two required for coupe, one required for sedan per front door.

#### Service Procedure:

1. Remove trim panel.

2. Remove water deflector to access lock rods.

3. With rods disengaged from anti-rattle clips, grasp clip with pliers and rotate 90 degrees to disengage.

4. Install new anti-rattle clips, reinstall rods.

5. Reinstall water deflector.

6. Reinstall trim panel.

Use most applicable Labour Operation and Time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.