Low and Reverse Clutch Housing Disassemble. Chevrolet Beretta 1996

For 1990-2009 cars

#### Tools Required

J 34008 Low-Reverse Clutch Housing Remover Installer

1. Using a flat blade screwdriver, remove the spacer retainer ring (647) for the low and reverse clutch housing (649) to case.
2. Install J 34008 into the low and reverse clutch housing assembly.
3. Push down on the handle in order to lock the tool into the clutch housing (649).
4. Lift the low and reverse clutch housing (649) out of the case.