Oil Pan Replacement. Chevrolet Beretta 1996

For 1990-2009 cars

### Removal Procedure

1. Remove the negative battery cable. Refer to

   Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

   in General Information.
2. Raise the vehicle. Refer to SECTION 0A.
3. Remove the right front tire and wheel assembly. Refer to SECTION 3B.
4. Remove the right engine splash shield. Refer to SECTION 10-4.
5. Drain the crankcase.
6. Remove the starter bracket at the block.
7. Remove the starter and lay it aside. Refer to Starter Motor Replacement in Engine Electrical.
8. Remove the transmission converter cover or the flywheel housing cover.
9. Remove the engine mount strut bracket. Refer to Engine Mount Strut Bracket Replacement .
10. Remove the oil level sensor.
11. Remove the oil pan bolts.
12. Remove the oil pan nuts.
13. Remove the oil pan.
14. Clean the sealing surfaces on the pan, cylinder case and front cover. Make sure that the old RTV is removed from the blind attaching holes.

### Installation Procedure

1. Place a 2 mm diameter bead of GM P/N 1052914 RTV sealer or equivalent to the oil pan sealing surface, except at the rear seal mounting surface.
2. Using a new oil pan rear seal, apply a thin coat of GM P/N 1052914 RTV sealer or equivalent on the ends down to the ears.
3. Install the oil pan.
4. Install the oil pan bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the oil pan nuts.

Tighten
Tighten the nuts to 10 N·m (89 lb in).

6. Install the oil level sensor.
7. Install the engine mount strut bracket. Refer to Engine Mount Strut Bracket Replacement .
8. Install the starter. Refer to Starter Motor Replacement in Engine Electrical.
9. Install the transmission converter cover or flywheel housing cover.
10. Install the right engine splash shield. Refer to SECTION 10-4.
11. Install the right front tire and wheel assembly. Refer to SECTION 3B.
12. Lower the vehicle.
13. Fill the crankcase with engine oil.
14. Connect the negative battery cable.