SERVICE MANUAL UPDATE - SPEC. REVISION (NEW ARTWORK). Chevrolet Beretta 1992

For 1990-2009 cars

# SERVICE MANUAL UPDATE - SPEC. REVISION (NEW ARTWORK)

#### SUBJECT: TORQUE SPECIFICATION REVISION FOR LOWER ENGINE MOUNT STRUT

#### MODEL and YEAR: 1992-93 CORSICA AND BERETTA

#### APPLICATION:

----------- 1992-93 "L"series with: 2.2L (VIN 4 - RPO LN2) 2.3L (VIN A - RPO LGO) 3.1L (VIN T - RPO LHO)

This is a service manual update to Sections 6A2, 6A5, 6A6 and 6A7.

The torque specification for the lower engine mount strut has been revised. Refer to the artwork on the following pages:

1992 L-car, 6A2-10, Figure 8 - Update with Figure 1. 1992 L-car, 6A5-14, Figure 12 - Update with Figure 2. 1992 L-car, 6A7-11, Figure 11 - Update with Figure 1. 1993 L-car, 6A7-12, Figure 12 - Update with Figure 1.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.