DELAYED NEUTRAL TO DRIVE ENGAGEMENT. Chevrolet Beretta 1988

For 1990-2009 cars

# DELAYED NEUTRAL TO DRIVE ENGAGEMENT

#### Model and Year: 1988 CELEBRITY, CAVALIER, CORSICA, BERETTA WITH THM 125/125C TRANSAXLE

A new Forward Clutch Housing and Thrust Washer entered production November 3, 1987 (Julian date 344). The Forward Clutch Housing (refer to 624 and 636 Figure 1) contains a stamped channel which increases forward clutch feed providing a shorter neutral to drive engagement.

If during repairs to an original designed forward clutch housing, replacement of the original plastic thrust washer is needed it may be replaced with an interim design metal thrust washer, P/N 8652759. This interim thrust washer does not contain dimples on both sides of its inside surface and will not fit the new forward clutch housing mentioned in this bulletin. . Whenever a new Forward Clutch Housing is used in previous model THM 125/125C transaxles, the new Powder Metal Bronze Thrust Washer must be used. The previous plastic Thrust Washer will not fit the new assembly. The latest design Powder Metal Washer is included in the package and can be identified by a dimple on both sides of the inside surface.

Package No. Package Description ----------- ------------------- 8664982 Forward Clutch Housing and Thrust Washer

8664762 New Thrust Washer (dimples inside surface)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.