POWER STEERING FLUID LOSS AT LOW AMBIENT TEMPERATURE. Chevrolet Beretta 1988

For 1990-2009 cars

# POWER STEERING FLUID LOSS AT LOW AMBIENT TEMPERATURE

#### Model and Year: 1988 BERETTA, CORSICA WITH 2.8L V6 ENGINE

Some 1988 Beretta, corsica models with 2.8L V-6 engines (RPO LB6) assembled prior to VIN breakpoints indicated below by assembly plant, may exhibit power steering fluid loss from the power steering cooling pipe inlet hose at low ambient temperatures (O degrees Fahrenheit or below).

Plant VIN Breakpoint ----- --------------- Wilmington JY561347 Linden JE557193

Vehicles exhibiting this condition may be repaired by replacement of the existing cooling pipe assembly and cooling pipe inlet hose with those currently in production following applicable shop manual procedure.

Parts required for this repair are indicated below and are now available from GMSPO.

Description Part Number ----------- ----------- Cooling Pipe Asm. 22531884 Cooling Pipe Inlet Hose 26001535

Parts are currently available.

Use applicable Labor Operation Number and Time.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.