GRUNT/SQUEAK SHIFT FROM PARK TO REVERSE/DRIVE. Chevrolet Beretta 1992

For 1990-2009 cars

# GRUNT/SQUEAK SHIFT FROM PARK TO REVERSE/DRIVE

#### Subject: GRUNT/SQUEAK SHIFTING FROM PARK TO REVERSE/DRIVE OR UNDER HEAVY ENGINE LOAD

#### Model and Year: 1992-93 CORSICA/BERETTA

THIS BULLETIN CANCELS AND SUPERSEDES DEALER SERVICE BULLETIN NO. 93-102-6 DATED FEBRUARY 1993. THE PARTS INFORMATION HAS BEEN UPDATED, VIN BREAKPOINTS INCLUDED AND A LABOR OPERATION NUMBER CHANGED. ALL COPIES OF 93-102-6 SHOULD BE DISCARDED.

ENGINE APPLICATION: 2.2L (VIN 4 - RPO LN2)

#### CONDITION:

--------- Some customers may comment about a grunt, squawk or squeak noise when shifting from park to reverse or drive. The same noise may also be heard during heavy engine load, such as quick acceleration. The noise will most likely occur in cold ambient temperatures or wet conditions.

#### CAUSE:

----- On 1992-93 vehicles, the lower engine mount strut rubber may move against its metal casting during the shift or heavy engine loads.

#### CORRECTION:

---------- Install revised lower engine mount strut, P/N 22595752, when diagnosis indicates the lower engine mount strut is at fault. Vehicles built after the following VIN breakpoint have the revised lower engine mount strut installed in production:

#### PLANT VIN

Wilmington PY244358

#### SERVICE INFORMATION:

#### IMPORTANT: Torque axis mounting systems allow more engine movement than other engine mounting systems. This movement may seem excessive but that is the design intent of the mounting system. Do NOT replace any torque axis mounts for movement unless there is damage to the mount or rubber.

Spray 3M silicone lubricant P/N 51135-08935 or equivalent on the lower engine mount strut between the rubber and metal.

#### NOTE: Use only silicone type lubricant between the rubber and metal surfaces. Any other lubricant will destroy the rubber making replacement of the lower engine mount strut necessary.

If the noise is gone, replace the lower engine mount strut with P/N 22595752 and submit labor operation T3368. The silicone lubricant will eliminate the condition for a short time only.

Parts are expected to be available on September 6,1993.

Labor Operation: T3368 Lower engine mount strut diagnosis and replace.

Labor Time: 0.4 hrs.

Failure Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.