FRT. DOOR HINGE PIN BREAKAGE INSTALL NEW P/N HINGE. Chevrolet Beretta 1988

For 1990-2009 cars

# FRT. DOOR HINGE PIN BREAKAGE INSTALL NEW P/N HINGE

#### Model and Year: 1987-88 L-CARS

#### TO: ALL CHEVROLET DEALERS

This bulletin cancels and replaces Dealer Service Bulletin 88-32 (Section 10) dated July, 1987, to increase labor time allowance. All copies of 88-32 should be discarded.

1987-88 Beretta, Corsica's that have been diagnosed as having a broken door hinge pin should be repaired by replacing both of the door hinges on the door of the vehicle that is affected.

New door hinges have been released and are available for these repairs as follows:

Hinge Asm. - Front Door Upper, P/N 10092242-3 (Right - Left) Hinge Asm. - Front Door Lower, P/N 10092244-5 (Right - Left)

The hinge replacement procedure is outlined in the Corsica/Beretta Service Manuals.

While replacing door hinges, the painted surfaces of the door and fender should be protected by tape. The door should be supported during removal and reinstallation by a helper and floor jack, with appropriate protection applied to the lift pad of the jack.

Use Labor Operation:

T1243 Both Hinges, Right Front Door 1.1 Hours T1244 Both Hinges, Left Front Door 1.1 Hours

ADD: Hinge Refinish and Material Allowance G B .4 Hours

Time includes door alignment.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.