LOOSE/MISSING HUB CAPS REPLACE WITH NEW COVERS. Chevrolet Beretta 1989

For 1990-2009 cars

# LOOSE/MISSING HUB CAPS REPLACE WITH NEW COVERS

#### VEHICLES AFFECTED: EARLY 1989 BERETTA GT

Some early 1989 Beretta GTs may experience loose and/or missing hub caps on the base rally wheel. This could include vehicles up to the following VIN numbers.

#### Plant VIN

Wilmington KY159340 Linden KE160712

If this condition occurs, replace the cover(s) with a new cover.

Labour Operation Number: E0022 Front Cover, Wheel Replace

E0023 Rear " " "

E0027 All

Labour Time : .2 Hour One or Both

.3 Hour All

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.