NO A/C COOLING DUE TO LOSS OF REFRIGERANT. Chevrolet Beretta 1993

For 1990-2009 cars

# NO A/C COOLING DUE TO LOSS OF REFRIGERANT

#### Subject: NO AIR CONDITIONING COOLING DUE TO LOSS OF REFRIGERANT

#### Model and Year: 1992-93 CORSICA AND BERETTA

YEAR BEGINNING VIN ENDING VIN ---- ------------- ---------- 1992 S.O.P E.O.P. 1993 S.O.P. Y219239

#### CONDITION:

--------- Loss of A/C cooling due to a refrigerant leak at the evaporator outlet. If leaks are encountered in the compressor condenser hose, refer to Dealer Service Bulletin 93-101-1A.

#### CAUSE:

----- Engine vibration and roll may cause stress on the evaporator eventually causing the evaporator outlet to crack resulting in the loss of the refrigerant charge.

#### CORRECTION:

---------- To correct this condition, a new evaporator should be installed as well as a new evaporator outlet tube. The new evaporator outlet tube is now equipped with a bracket that will need to be fastened to the front of dash. This new bracket will provide the strength necessary for the evaporator to withstand engine vibration and roll.

There is a service replacement kit, P/N 12355668, that includes a new evaporator, evaporator outlet tube and bracket, and a self drilling screw used to attach the bracket to the f ront of dash. To replace the evaporator, follow the procedure outlined in SECTION 1B of the appropriate service manual. To replace the evaporator outlet tube and bracket assembly, perform the following procedure.

1. Recover any refrigerant remaining in the a/c system.

2. Raise vehicle.

3. Remove evaporator outlet tube fitting at evaporator outlet.

4. Remove the old evaporator outlet tube.

5. Install the new evaporator outlet tube (lubricating new "O" rings) making sure that the bracket fits properly under the lip on the front of dash. (Refer to Figure 1)

6. Install the self drilling screw through the bottom side of the bracket. (This can be done by using a 1/4" extension in a 1/2" drill.)

7. Lower vehicle.

8. Evacuate and recharge A/C system.

9. Leak test.

Parts are expected to be available on May 24,1993.

#### WARRANTY INFORMATION:

Labor Operation: T3336 Labor Time: 1.7 hr Add A: Recover/Recharge A/C System: .7 hr Failure Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.