COOLING SYSTEM LEAK AT RADIATOR HOSES-NEW P/N CLAMP. Chevrolet Beretta 1988

For 1990-2009 cars

# COOLING SYSTEM LEAK AT RADIATOR HOSES-NEW P/N CLAMP

#### Model and Year: 1987-88 BERETTA, CORSICA WITH 2.0L OR 2.8L ENGINE

Some of the above vehicles may experience radiator hose leaks due to the hose clamps having insufficient clamping force.

This condition may be repaired by replacing the existing hose clamps with the following service part.

Part Number Part Name ----------- ----------- 10056745 Hose Clamp

These clamps can be used as service parts on both the upper and lower radiator hoses.

This condition may be present on any vehicle built prior to the following breakpoints.

Linden JE 291533

Wilmington JY 284984

Use applicable labor operation and time.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.