Volts Indicator Lamp Never On. Chevrolet Beretta 1996

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---

1

1. Disconnect the generator connector.
2. Connect fused jumper across terminal L (V6 VIN M) or terminal B (L4 VIN 4) and ground.
3. Turn the ignition switch to RUN.

Does the charge indicator light?

--

Go to Step 3

Go to Step 2

2

1. Check CKT 25, 39 and bulb for an open.
2. If OK, replace or exchange instrument cluster.

Is the repair complete?

--

System OK

--

3 | Repair or replace the generator. Refer to Generator Replacement or Generator Replacement . Is the repair complete? | -- | System OK | --