Valve Lifter Removal. Chevrolet Beretta 1996

For 1990-2009 cars

1. Remove the rocker arm cover. Refer to Valve Rocker Arm Cover Removal.
2. Remove the rocker arms and push rods. Refer to Valve Rocker Arm Cover Removal.
3. Remove the cylinder head. Refer to Cylinder Head Removal.
4. Remove the bolts that secure the lifter anti-rotation brackets.
5. Remove the anti-rotation brackets.
6. Remove the valve lifters from the lifter bore.
7. Inspect the valve lifter for the following conditions:

• | Lifter wear

• | Lifter scuffing

• | Loose roller shaft

8. Inspect the valve lifter bore in the engine block for wear and scuffing.
9. Inspect the roller for freedom of movement.
10. Inspect the roller surface for flat spots and pitting.