INFORMATION ON OIL FILTER SIZE IN OWNERS MANUAL PARTS BOOK. Chevrolet Beretta 1987

For 1990-2009 cars

# INFORMATION ON OIL FILTER SIZE IN OWNERS MANUAL PARTS BOOK

#### SUBJECT: CORRECT OIL FILTER (INFORMATION ON SIZE OF FILTER IN OWNERS MANUAL, PARTS BOOK)

#### VEHICLES AFFECTED: 1987-91 CHEVROLET L-CAR W/2/8L OR 3.1L

This bulletin advises dealers and customers of the correct replacement oil filter for the specified vehicles. Disregard information contained in the 1987-91 Corsica/Beretta Owners Manuals and Parts Catalogues showing the AC-TYPE PF-51 as the replacement oil filter. The proper replacement oil filter for the specified vehicles is an AC TYPE PF-40. The AC TYPE PF-51 extends below the suspension and may be damaged by stones, rocks, or road hazards. The AC TYPE PF-40 is shorter and does not extend below the suspension.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.