Crankshaft Front Cover Oil Seal Replacement. Chevrolet Beretta 1996

For 1990-2009 cars

### Removal Procedure

1. Remove the crankshaft pulley and the crankshaft pulley hub. Refer to Crankshaft Balancer and Hub Replacement .
2. Remove the oil seal by prying it out with a large screwdriver. Do no damage the seal seat or the crankshaft.

### Installation Procedure

#### Tools Required

J 35468 Seal Centering Tool.

1. Install the crankshaft pulley and the crankshaft pulley hub. Refer to Crankshaft Balancer and Hub Replacement .
2. Install the front cover oil seal using J 35468 .