INFO. ON REPLACEMENT OF GUIDE LOOP COVERS ON FRONT SEAT BELT. Chevrolet Beretta 1992

For 1990-2009 cars

# INFO. ON REPLACEMENT OF GUIDE LOOP COVERS ON FRONT SEAT BELT

#### SUBJECT: INFORMATION ON REPLACEMENT OF GUIDE LOOP COVERS ON FRONT SEAT BELTS

#### VEHICLES AFFECTED: 1991-93 "L" MODELS

If one of the guide loop covers on the front seat belts of some 1991-93 "L" cars becomes broken or is found to be missing, a replacement guide loop cover is available separate from the seat belt assembly itself. The seat belt assembly DOES NOT need to be replaced when there is a problem with the guide loop cover.

1. Remove bolt holding the guide loop to the pillar using J23457 -seat belt anchor tool.

2. Remove the guide loop cover from the guide loop.

3. Install new guide loop cover.

4. Install bolt to pillar, tighten to 42 N.m (31 lbs. ft.) using J23457 - seat belt anchor tool, and snap new guide loop cover into place over the guide loop and anchor bolt.

Part Number Description ----------- ----------- 22578473 Guide loop cover, very dark sapphire 22578474 Guide loop cover, medium beige 22578475 Guide loop cover, garnet red 22578476 Guide loop cover, medium dark gray 22578477 Guide loop cover, medium gray

Labour Operation Number: Right C9050 Left C9051 Labour Time: .2 hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.