Differential Carrier Complete Disassemble. Chevrolet Beretta 1996

For 1990-2009 cars

#### Tools Required

J 33381-A Final Drive Unit Remover and Installer

1. Remove J 33381-A from the differential carrier (673) and final drive assembly (678).
2. Remove the final drive internal gear (673).
3. Remove the thrust bearing (674) connecting the sun gear to the internal gear (673).
4. Remove the sun gear (675).
5. In some models, remove the thrust bearing (676) connecting the sun gear to the final drive carrier (678).