DTC P0724 Brake Switch Circuit High Input. Chevrolet Beretta 1996

For 1990-2009 cars
Automatic Transmission Components
Automatic Transmission Controls Schematics
OBD II Symbol Description Notice
Handling ESD Sensitive Parts Notice

### Circuit Description

The Torque Converter Clutch (TCC) brake switch indicates brake pedal status to the Powertrain Control Module (PCM). The normally-closed switch supplies battery voltage on circuit 422 to the PCM. Applying the brake pedal opens the brake switch, interrupting voltage to the PCM. While the brake pedal is not applied, the PCM receives constant voltage. If the PCM receives 0 volts at the brake switch input with the Torque Converter Clutch engaged, the PCM de-energizes the Torque Converter Clutch Solenoid Valve (TCC Sol. Valve).

When the PCM detects a closed brake switch (stuck OFF) during decelerations, then DTC P0724 sets. DTC P0724 is a type D DTC.

### Conditions for Setting the DTC

• | No Vehicle Speed Sensor Assembly DTC P0502

• | The vehicle speed is greater than 32 km/h (20 mph) for at least 6 seconds,

| then the vehicle speed is 8-32 km/h (5-20 mph) for 4 seconds,

| then the vehicle speed remains less than 8 km/h (5 mph).

• | The above conditions must occur 7 times without a brake switch status change.

### Action Taken When the DTC Sets

The PCM does not illuminate the Malfunction Indicator Lamp (MIL).

### Conditions for Clearing the MIL/DTC

A scan tool can clear the DTC from the PCM history. The PCM clears the DTC from the PCM history if the vehicle completes 40 warm-up cycles without a failure reported.

### Diagnostic Aids

• | Inspect the TCC brake switch for proper adjustment.

• | Inspect the wiring for poor electrical connections at the PCM. Inspect the wiring for poor electrical connections at the TCC brake switch connector. Look for the following conditions:

- | A bent terminal

- | A backed out terminal

- | A damaged terminal

- | Poor terminal tension

- | A chafed wire

- | A broken wire inside the insulation

• | When diagnosing for an intermittent short or open condition, massage the wiring harness while watching the test equipment for a change.

### Test Description

The numbers below refer to the Step numbers on the diagnostic table.

1. If you disconnect the brake switch connector and observe a brake switch status change, then a brake switch problem is the only possible cause of the DTC.

2. If the brake switch is properly adjusted, then you must replace the brake switch.

3. An unchanging brake switch status (OFF) in Step 2 indicates a possible short to power in circuit 422. This step inspects circuit 422 for a short to power. If you find a short, repair the circuit.

4. Replace the PCM only after you have completed the preceding diagnostic steps.

#### DTC P0724

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Powertrain On-Board Diagnostic (OBD) System Check performed? | -- | Go to Step 2 | Go to Powertrain On Board Diagnostic (OBD) System Check

2

1. Install the scan tool.
2. With the engine OFF, turn the ignition switch to the RUN position.

Important: Before clearing the DTCs, use the scan tool in order to record the Failure Records for reference. The Clear Info function will erase the data.

3. Record the DTC Failure Records.
4. Select scan tool TCC brake switch.
5. Disconnect the brake switch connector.

Did the brake switch status change from OFF to ON?

--

Go to Step 3

Go to Step 4

3 | Replace the brake switch. Refer to Brake and Clutch Pedal Switches, Section 8. Is the replacement complete? | -- | Go to Step 6 | --
4 | Inspect circuit 422 for a short to power. Refer to Troubleshooting Procedures, Section 8. Did you find and correct the condition? | -- | Go to Step 6 | Go to Step 5
5 | Replace the PCM. Refer to Powertrain Control Module/EEPROM Replacement/Programming , Section 6. Is the replacement complete? | -- | Go to Step 6 | --

6

In order to verify your repair, perform the following procedure:

1. Select DTC.
2. Select Clear Info.
3. Operate the vehicle under the following conditions:

• | Turn the ignition switch to the RUN position.

• | Apply the brake pedal for 2 seconds or more.

4. Select Specific DTC. Enter DTC P0724.

Has the test run and passed?

--

System OK

Begin the diagnosis again. Go to Step 1