Crankshaft Pulley and Hub Removal. Chevrolet Beretta 1996

For 1990-2009 cars

### Crankshaft Pulley Removal Procedure

1. Remove the crankshaft pulley bolts.
2. Remove the hub bolt of the crankshaft pulley.
3. Remove the crankshaft pulley.

### Crankshaft Pulley Hub Removal Procedure

#### Tool Required

J 24420-B Crankshaft Pulley Hub Puller

1. Remove the crankshaft pulley.
2. Position the J 24420-B onto the crankshaft pulley hub.
3. Turn the puller screw clockwise. This will remove the hub from the crankshaft.