Driven Sprocket Support Components Assemble. Chevrolet Beretta 1996

For 1990-2009 cars

Important: The ends of the scarf cut seal ring must overlap each other as shown in the diagram.

1. Lubricate new seals (604) with TRANSJEL™ or equivalent. Affix the new seals onto the driven sprocket support assembly (602).
2. The seal joints may be positioned randomly around the support assembly (602).
3. Use TRANSJEL™ or equivalent in order to insert the thrust washer (605) onto the support assembly (602).
4. Install the driven sprocket support assembly (602) into the case.