Case Cover Components Disassemble. Chevrolet Beretta 1996

For 1990-2009 cars

#### Tools Required

• | J 23129 Axle Seal Remover

• | J 6125-1B Slide Hammer

1. Remove the 1-2 accumulator piston assembly (421) and the pin (422) from the case cover (401).
2. Remove the 1-2 accumulator piston seal (420) from the 1-2 accumulator piston (421).
3. Use J 23129 and J 6125-1B in order to remove the left drive axle seal (31) from the case cover (401).
4. Use a small flat blade screwdriver in order to unlock the electrical connector tabs. Remove the electrical connector (408).
5. Remove the connector seal (407) from the connector (408).
6. Remove the manual valve (406) from the case cover (401).