Intermediate Servo Replacement. Chevrolet Beretta 1996

For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Support the vehicle. Refer to General Vehicle Lifting and Jacking in General Information.
2. Remove the oil pan and the gasket.
3. Remove the oil pan filter and the seal.
4. Remove the reverse oil pipe retainer.
5. Remove the governor oil pipe retainer.
6. Remove the intermediate band servo cover.
7. Remove the intermediate band servo cover gasket.
8. Remove the accumulator exhaust valve.
9. Remove the accumulator exhaust spring.
10. Remove the intermediate servo piston inner ring.
11. Remove the snap ring.
12. Remove the servo piston.
13. Remove the intermediate servo piston outer ring.
14. Remove the intermediate band servo piston spring.
15. Remove the piston spring retainer.
16. Remove the piston pin.
17. Remove the intermediate band servo pin seal.

### Installation Procedure

1. Install the intermediate band servo pin seal.
2. Install the intermediate band piston pin.
3. Install the piston spring retainer.
4. Install the piston spring.
5. Install the intermediate servo piston outer ring.
6. Install the servo piston.
7. Install the snap ring.
8. Install the intermediate servo piston inner ring.
9. Install the accumulator exhaust spring.
10. Install the accumulator exhaust valve.
11. Install the intermediate band servo cover gasket.
12. Install the intermediate band servo cover.
13. Install the governor oil pipe retainer.
14. Install the reverse oil pipe retainer.
15. Install the oil pan, the oil pan filter, and the seal.
16. Lower the vehicle.
17. Adjust the oil level.