Shift Speed. Chevrolet Beretta 1996

For 1990-2009 cars

#### Hydra-Matic 4T60-E Shift Speed Chart

Transmission Model | 6WFW
--- | ---
Vehicle Series | L
Engine Displacement | 3.1L
Engine RPO Code | L82
Engine VIN Code | M
Overall Axle Ratio | 2.93
Final Drive Ratio | 3.29
Drive/Driven Sprocket Teeth | 37/33
Minimum Throttle 1-2 Upshift | 9
Wide Open Throttle 1-2 Upshift | 43
Minimum Throttle 2-3 Upshift | 20
Wide Open Throttle 2-3 Upshift | 82
Minimum Throttle 3-4 Upshift | 32
Wide Open Throttle 3-4 Upshift | N/A
Minimum TCC Apply - Third Gear | 45
Minimum TCC Apply - Fourth Gear | 48
N/V Ratio - Third Gear/TCC On | 46
N/V Ratio - Fourth Gear/TCC On | 32

- N/V Ratio = Engine RPM to Vehicle Speed Ratio
- N/A = Not Available
- Speeds are indicated in Miles Per Hour (MPH). MPH = Km/h x 1.609