Low and Reverse Pipes and Cup Plug Replacement. Chevrolet Beretta 1996

For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Support the vehicle. Refer to General Vehicle Lifting and Jacking in General Information.
2. Remove the oil pan and the gasket.
3. Remove the oil pan filter and the seal.
4. Remove the reverse oil pipe.
5. Remove the back-up ring seal.
6. Remove the reverse pipe to case O-ring.
7. Remove the low and reverse cup plug assembly. Use the screw extractor.

### Installation Procedure

1. Install the low and reverse cup plug assembly.
2. Install the reverse pipe to case O-ring.
3. Install the new back up ring seal.
4. Install the reverse the oil pipe.
5. Install the oil pan filter and the seal.
6. Install the oil pan and the gasket.
7. Lower the vehicle.
8. Check the oil level.