Valve Lifter Installation. Chevrolet Beretta 1996

For 1990-2009 cars

Notice: If the valve lifters and anti-rotation brackets are not installed properly, the valve lifters, the anti-rotation brackets, and the engine could be damaged.

Important: When installing new valve lifters, coat the lifters with camshaft assembly lube (GM P/N 1052365) or equivalent.

1. Install the valve lifters in the lifter bores.

• | Align the flat sides (top) of the lifters with the flat sides of the anti-rotation brackets.

• | When properly aligned, the flat side of each lifter is aligned parallel to the anti-rotation bracket.

• | The roller at the bottom of each lifter is aligned parallel to the camshaft lobe.

2. Install the anti-rotation brackets on the valve lifters.
3. Install the screws that retain the anti-rotation brackets.

Tighten
Tighten the anti-rotation bracket screws to 11 N·m (97 lb in). Refer to

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

in General Information.
4. Install the cylinder head. Refer to Cylinder Head Installation.
5. Install the rocker arms and push rods. Refer to Valve Rocker Arm Installation.
6. Install the rocker arm cover. Refer to Valve Rocker Arm Cover Installation.