Volts Indicator Lamp Always On. Chevrolet Beretta 1996

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---

1

1. Disconnect the generator connector.
2. Turn the ignition switch to RUN.

Does the charge indicator remain lit?

--

Go to Step 3

Go to Step 2

2 | Repair or replace the generator. Refer to Generator Replacement or Generator Replacement . Is the repair complete? | -- | System OK | --
3 | Check CKT 25 for a short to ground. If OK, replace or exchange the instrument cluster. Is the repair complete? | -- | System OK | --