Starting and Charging Components. Chevrolet Beretta 1996

For 1990-2009 cars

Name | Location | Locator View | Connector End View | Group No.
--- | --- | --- | --- | ---
Battery | LH fender in engine compartment | 8A-201-9 Fig. 18 | -- | --
Clutch Pedal Position Switch | LH front I/P | 8A-201-18 Fig. 35 | -- | --
Fuse Block | LH front I/P | 8A-201-18 Fig. 35 | -- | --
Fusible Link B | Lower front of engine | 8A-201-9 Fig. 17 | -- | --
Fusible Link C | Lower front of engine | 8A-201-9 Fig. 17 | -- | --
Generator | Rear of engine | 8A-201-3 Fig. 6 | 202-42 | --
Ignition Switch | RH steering column | 8A-201-26 Fig. 52 | 202-43 | --
Inline GEN Fuse A | LH rear corner of engine compartment | 8A-201-25 Fig. 49
Instrument Cluster | LH center I/P | 8A-201-19 Fig. 38 | 202-18 | --
Transaxle Range Switch (VIN 4) | Rear of engine | 8A-201-2 Fig. 4 | 202-43 | --
Transaxle Range Switch (VIN M) | Rear of engine | 8A-201-2 Fig. 4 | 202-23 | --
Starter Motor | LH front of engine/transaxle | 8A-201-3 Fig. 5 | -- | --
Starter Solenoid | LH front of engine/transaxle | 8A-201-3 Fig. 5 | -- | --
CONNECTORS:
C100 (42 Cavities) | LH front of dash | 8A-201-7 Fig. 14 | 202-0 | --
GROUNDS:
G101 | LH front of engine/transaxle | 8A-201-3 Fig. 5 | -- | --
G106 | LH front of engine compartment | 8A-201-9 Fig. 18 | -- | --
SPLICES:
S113 | Engine compartment front of dash | 8A-201-5 Fig. 10 | -- | --
S201 | Lower steering column | 8A-201-20 Fig. 39 | -- | --
S208 | Engine compartment front of dash | 8A-201-5 Fig. 10 | -- | --
S227 | RH I/P | 8A-201-11 Fig. 22 | -- | --
S233 | LH rear of engine compartment | 8A-201-10 Fig. 19 | -- | --
S290 | Lower steering column | 8A-201-20 Fig. 39 | -- | --