2-3 Shift Soft, Slips, or Early. Chevrolet Beretta 1996

For 1990-2009 cars

Checks | Cause
--- | ---
Oil Level | Incorrect level
TV Cable | Misadjusted, unhooked, bound, or broken (22)
Manual Linkage (701-704) | Misadjusted
Oil Pressure | Check for causes of high or low oil pressure

Intermediate Servo (128-137)

• | The Piston to case oil seal is damaged (132)

• | The servo piston is damaged

• | The servo bore in the case is damaged (15)

Accumulator Exhaust Check Valve (125, 126) | Not seating in the case

Spacer Plate (20)

• | The direct clutch feed orifice is plugged or restricted

• | The spacer plate or the gaskets are leaking, damaged, or incorrectly installed (19, 20)

• | Incorrect spacer plate (20)

Checkball #5 (16) | Not seating or missing

Case Cover (401)

• | Porosity is in the direct clutch case cover passage

• | Case cover gaskets are incorrect (25, 416)

• | The driven sprocket support passages are interconnected, leaking, or restricted (602)

• | The driven sprocket support oil seal rings are damaged or are missing (604)

• | The sleeve is loose or is out of position (601)

Direct Clutch (608-617)

• | A leaking checkball (609)

• | A damaged checkball capsule (610)

• | Damaged or missing seals (612-614)

• | A cracked or damaged housing or piston (610, 615)

• | A missing or incorrect apply ring (616)

• | The wrong number of clutch plates (618)