Brake Pressure Modulator Valve Bracket Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Turn the ignition switch to the OFF position.
2. Remove the EBCM/BPMV assembly (1) from the lower BPMV bracket (2). Refer to Brake Pressure Modulator Valve Replacement.
3. Remove the brake pressure modulator valve bracket nuts (4).
4. Remove the brake pressure modulator valve bracket (2).

### Installation Procedure

1. Install the brake pressure modulator valve bracket (2).
2. Install the brake pressure modulator valve bracket nuts (4).

Tighten
Tighten the nuts to 27 N·m (20 lb ft).

3. Install the EBCM/BPMV assembly (1) to the lower BPMV bracket (2). Refer to Brake Pressure Modulator Valve Replacement.
4. Perform the ABS Bleed Procedure.
5. Perform the ABS Diagnostic System Check.