Rear Compartment Lid Weatherstrip Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Peel the weatherstrip from the gutter flange. Move the weatherstrip in the following direction:

1.1. | Toward the lower corners

1.2. | Around the complete opening

2. Clean all of the adhesive from the pinch-weld flange.

### Installation Procedure

1. Apply a bead of weatherstrip adhesive to the following areas:

1.1. | The edge of the pinch-weld flange

1.2. | Around the entire perimeter of the rear compartment opening

2. Install the center of the weatherstrip onto the gutter flange. Begin at the forward center of the opening between the flanges.
3. Push down by hand the weatherstrip over the entire area. This process ensures the proper seating of the weatherstrip.