DTC P1336 Crankshaft Position (CKP) System Variation Not Learned. Chevrolet PJJ 2000

For 1990-2009 cars

### Circuit Description

In order to detect an engine misfire at higher engine speeds, the Powertrain Control Module (PCM) must know of any variation between the crankshaft sensor pulses. Most variations are due to the machining of the crankshaft reluctor wheel, however, other sources of variation are also possible. A crankshaft position system variation learn procedure must be performed any time that you perform the following service procedures, regardless of whether or not the DTC P1336 is set:

• | PCM replacement

• | Engine replacement

• | Crankshaft replacement

• | Crankshaft balancer replacement

• | Crankshaft position sensor replacement

• | Any engine repairs which disturbs the crankshaft/harmonic balancer to the crankshaft position sensor relationship

The PCM measures the variations and then calculates compensation factors needed in order to enable the PCM to accurately detect an engine misfire at all speeds and loads. A scan tool must be used to command the PCM to learn these variations. A DTC P1336 will set if the PCM has not had the crankshaft position system variation learn procedure performed due to replacement or a reprogramming.

### Conditions for Setting the DTC

• | No crank or cam sensor DTCs.

• | The PCM has not successfully learned the crankshaft position system variation.

### Action Taken When the DTC Sets

• | The malfunction indicator lamp (MIL) will illuminate.

• | The PCM will record the operating conditions at the time during which the diagnostic fails. This information will store in the Freeze Frame and Failure Records buffers.

• | A history DTC stores.

### Conditions for Clearing the MIL/DTC

• | The MIL will turn OFF after three consecutive ignition cycles in which the diagnostic runs without a fault.

• | A history DTC will clear after 40 consecutive warm-up cycles without a fault.

• | Use a scan tool to clear the DTCs.

### Diagnostic Aids

Important: Before performing the Crankshaft Position System Variation Learning Procedure always set the vehicle parking brake and block the drive wheels in order to prevent personal injury. Release the throttle immediately when the engine starts to decelerate in order to eliminate over revving the engine. Once the learn procedure is completed, the control module will return engine control to the operator and the engine will respond to the throttle position.

DTC P1336 will only set if the PCM has not learned the crankshaft position system variation. The PCM only needs to learn this variation once per life cycle of the vehicle unless the crank sensor to crankshaft relationship is disturbed. Removing a part for inspection and then reinstalling the same part is considered a disturbance.

The crankshaft position system variation learn procedure must be performed when replacing the PCM in order to clear the DTC P1336. The crankshaft position system variation learn procedure is also required when the following service procedures have been performed, regardless of whether or not DTC P1336 is set:

• | PCM replacement

• | Engine replacement

• | Crankshaft replacement

• | Crankshaft balancer replacement

• | Crankshaft position sensor replacement

• | Any engine repairs which disturbs the crankshaft/harmonic balancer to crankshaft position sensor relationship.

A fully warmed up engine is critical to learning the variation correctly. If a valid learn occurs, no other learns can be completed on that ignition cycle.

If the engine cuts out before the specified learn procedure engine speed or at normal fuel cut-off RPM, the PCM is not in the learn procedure mode. Review the crankshaft position system variation learn procedure and re-enable the learn procedure. Verify that the scan tool displays Test in Progress.

#### Excessive Crankshaft Variation Symptom

Scan Tool Display | Possible Causes
--- | ---
Factors out of range | The reluctor wheel-machining quality, a run out, or an incorrect air gap.
Opposing factors out of range | Disturbance-Noise on the crank sensor circuit. Reattempt the Learn Procedure.
Sum out of range | The engine is too cold. Reattempt the Learn Procedure.
Crank pulse count error. | Crank or Cam sensor DTCs is set. Repair the affected DTC first

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. The engine temperature is critical in order to properly learn the crankshaft position system variation. Failure to properly warm the engine before performing this procedure will result in an inaccurate measurement of the crankshaft position system learn variation. The PCM learns this variation as the engine is decelerating and then allows the engine control to be returned to the operator. All accessories must be turned OFF when learn the crankshaft position system angle variation. If the A/C is not disabled when the learn procedure is enabled, the PCM will disable the A/C. When the PCM is ready to allow the learn procedure to run, the scan tool will display Test in Progress.

2. Being unable to learn the crankshaft position system learn variation indicates that the variation is out of range. Using the excessive crankshaft variation troubleshooting will help in order to diagnose the area where the problem lies.

#### DTC P1336 - Crankshaft Position System Angle Variation Not Learned

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Powertrain On-Board Diagnostic (OBD) System Check? | -- | Go to Step 2 | Go to Powertrain On Board Diagnostic (OBD) System Check
2 | Perform the Crankshaft Position System Variation Learn procedure. Refer to Crankshaft Position System Variation Learn . Does the scan tool indicate that the crankshaft position system variation has been learned? | -- | Go to Step 4 | Go to Step 3

3

1. Turn OFF the ignition.
2. Inspect the crank sensor to crankshaft relationship. Refer to the Excessive Crankshaft Variation Symptom Table.
3. If a problem is found, repair as necessary.

Did you find and correct the condition?

--

Go to Step 4

Go to Diagnostic Aids

4

1. Use a scan tool to clear the DTCs.
2. Turn OFF the ignition for 30 seconds.
3. Operate the vehicle within the Conditions for Running the DTC as specified in the supporting text.

Does the DTC reset?

--

Go to Step 2

System OK