Door Lock Striker Adjustment. Chevrolet PJJ 2000

For 1990-2009 cars

Notice: Striker alignment is a crucial part of door latch operation. Do not use the door striker to adjust the door to the vehicle. Failure to properly adjust the striker can result in damage to the door latch and the striker.

1. Loosen the striker bolts (2).
2. Attach the striker bolts (2) snugly in order to ensure that the striker (1) is still movable.
3. Pull on the outside handle.
4. Gently push the door against the body in order to ensure that the striker (1) allows a flush fit.
5. Slowly open the door.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

6. Tighten the bolts (2).

Tighten
Tighten the bolts (2) to 24 N·m (18 lb ft).

7. Touch up any exposed or unpainted surface on the lock pillar.