Auxiliary Outlets Inoperative. Chevrolet PJJ 2000

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Inspect the 20A AUX PWR/CIG fuse for an open. Is fuse open? | -- | Go to Step 2 | Go to Step 3

2

1. Remove auxiliary power outlet.
2. Test terminal A for continuity to ground.

Is ground present?

--

Go to Step 4

--

3

1. Reinstall fuse.
2. Test terminal A for positive battery voltage.

Is battery voltage present?

--

Go to Step 5

Go to Step 7

4 | Repair short to ground in CKT 40. Is repair complete? | -- | System OK | --
5 | Test terminal C for continuity to ground. Is ground present? | -- | Go to Step 6 | Go to Step 8
6 | Replace auxiliary outlet. Is repair complete? | -- | System OK | --
7 | Repair open in CKT 40. Is repair complete? | -- | System OK | --
8 | Repair open in CKT 150. Is repair complete? | -- | System OK | --