Fog Lamp Switch Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Disable the SIR system. Refer to Disabling the SIR System in SIR.
2. Remove the trim plate from the instrument panel cluster (1). Refer to Trim Replacement - IP Lower Center in Instrument Panel, Gauges, and Console.
3. Disconnect the electrical connectors.
4. Press tabs to remove the fog lamp switch (3).

### Installation Procedure

1. Install the fog lamp switch (3).
2. Connect the electrical connectors.
3. Install the trim panel to the instrument panel cluster (1). Refer to Trim Replacement - IP Lower Center in Instrument Panel, Gauges, and Console.
4. Enable the SIR system. Refer to Trim Plate Bezel Replacement - IP Cluster in SIR.