Instrument Cluster Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Disable the SIR system. Refer to Disabling the SIR System in SIR.
2. Remove the instrument panel trim pad. Refer to Trim Pad Replacement - IP.
3. Remove the instrument panel trim plate. Refer to Trim Plate Bezel Replacement - IP Cluster.
4. Remove the screws (1) from the top of the cluster.
5. Remove electrical connector (3).
6. Pull the cluster rearward.
7. Remove the cluster.

### Installation Procedure

1. Connect the electrical connector (3).
2. Install the cluster to the instrument panel.
3. Install the screws (1) at the top of the cluster.

Tighten
Tighten the screws to 2 N·m (18 lb in).

4. Install the instrument panel trim plate. Refer to Trim Plate Bezel Replacement - IP Cluster.
5. Install the instrument panel trim pad. Refer to Trim Pad Replacement - IP.
6. Enable the SIR system. Refer to Enabling the SIR System in SIR.