Backup Lamp Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Disconnect the lamp sockets (5).
2. Remove the assembly retaining nuts (1) from behind the rear compartment lid.
3. Remove the assembly.
4. Pull the back-up lamp bulb from the socket.

### Installation Procedure

1. Install the assembly.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the retaining nuts (1).

Tighten
Tighten the retaining nuts to 5 (44 lb in).

3. Install the bulbs.
4. Install the sockets (5).