Cargo Lamp Switch Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the rear window panel trim. Refer to Trim Panel Replacement - Rear Window in Body Rear End.
2. Disconnect the electrical connector.
3. Slide the switch (1) out from the bracket.

### Installation Procedure

1. Connect the electrical connector.
2. Install the switch (1).
3. Install the rear window panel trim. refer to Trim Panel Replacement - Rear Window in Body Rear End.