Fastener Tightening Specifications. Chevrolet PJJ 2001

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Heater Control to IP | 2 N·m | 18 lb in
Compartment to IP | 2 N·m | 18 lb in
Console and Floor Pan to Console Bracket | 2 N·m | 18 lb in
Convenience Center to IP | 6 N·m | 53 lb in
IP Accessory Trim Plate | 2 N·m | 18 lb in
IP Cluster to IP | 2 N·m | 18 lb in
IP Cluster Trim Plate | 2 N·m | 18 lb in
IP End Cap Screws to IP | 2 N·m | 18 lb in
IP to Tie Bar Bolts | 2 N·m | 18 lb in
IP to Tie Bar Nuts | 10 N·m | 89 lb in
IP Upper Pad to Lower IP | 2 N·m | 18 lb in
Neutral Start Switch | 4 N·m | 35 lb in
Rear Window Defroster Relay to IP | 2 N·m | 18 lb in
Sound Insulators | 2 N·m | 18 lb in