Engine Coolant Temperature Sensor Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

Notice: Use care when handling the coolant sensor. Damage to the coolant sensor will affect the operation of the fuel control system.

1. Turn OFF the ignition switch.
2. Drain the coolant system. Refer to Cooling System Draining and Filling in Engine Cooling.
3. Disconnect the ECT sensor electrical connector.
4. Carefully remove the ECT sensor.

### Installation Procedure

1. Coat only the threads of the ECT sensor with thread sealer.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the ECT sensor in the engine.

Tighten
Tighten the ECT sensor to 23 N·m (17 lb in).

3. Connect the ECT sensor electrical connector.
4. Refill the engine coolant system. Refer to Cooling System Draining and Filling in Engine Cooling.