Courtesy Lamps Always On. Chevrolet PJJ 2001

For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you perform the Diagnostic System Check - Lighting Systems? | Go to Step 2 | Go to Diagnostic System Check - Lighting Systems
2 | Use the Scan Tool in order to command the courtesy lamps OFF. Do the courtesy lamps turn OFF? | Go to Step 4 | Go to Step 3
3 | Test for a short to ground in the interior lamp control circuit. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | System OK | Go to Step 7

4

Test for a short to ground in each of the door jamb switch signal circuits. Refer to

#### Power Door Locks with Keyless Entry

Power Door Systems Components
Power Door Locks Circuit Description
Power Door Locks with Keyless Entry
G302
G304 (2 of 2)
Power Door Locks with Keyless Entry
Power Door Locks with Keyless Entry
Handling ESD Sensitive Parts Notice
in Door Systems, Circuit Testing and Wiring Repairs in Wiring Systems.

Did you find and correct the condition?

System OK

Go to Step 5

5

Test each door jamb switch for proper operation. Refer to the following:

• | Open switch with the door closed

• | Closed switch with the door open

Refer to Circuit Testing and Wiring Repairs in Wiring Systems.

Did you find a malfunctioning door jamb switch?

Go to Step 6

Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems

6 | Replace the malfunctioning door jamb switch. Refer to Door Jamb Switch Replacement in Doors. Is the repair complete? | System OK | --
7 | Important: Perform the set up procedure for the body control module. Replace the body control module. Refer to Body Control Module Replacement . Did you complete the replacement? | System OK | --