Radio Antenna Module Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the rear package trim panel. Refer to Rear Window Trim Panel Replacement .
2. Disconnect the electrical connectors (3).
3. Remove the retaining screws (2).
4. Remove the module.

### Installation Procedure

1. Install the module.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the retaining screws (2).

Tighten
Tighten the retaining screws to 2 N·m (18 lb in).

3. Connect the electrical connectors (3).