Speaker Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Door Trim Panel Replacement in Doors.
2. Disconnect the electrical connector (2).
3. Remove the bolts (3).
4. Remove the front door speaker.

### Installation Procedure

1. Install the front door speaker.
2. Install the bolts (3).
3. Connect the electrical connector (2).
4. Install the door trim panel. Refer to Door Trim Panel Replacement in Doors.