Front Lower Control Arm Bushing Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

#### Tools Required

• | J 21474-4 Control Arm Bushing Set

• | J 21474-18 Nut

• | J 21474-19 Bolt

• | J 21474-27Bolt

• | J 41211 Front Control Arm Bushing Kit

• | J 41397 Lower Control Arm Bushings Remover/Installer

1. Remove the lower control arm. Refer to Lower Control Arm Replacement.
2. Secure the lower control arm in a vice.

Important: Apply J 23444 A (or equivalent high pressure lubricant) to the threads of the J 21474-19 Bolt.

3. Assemble the following bushing removal tools as shown:

• | J 21474-19 Bolt

• | The remover/installer from the J 41397Lower Control Arm Bushings Remover/Installer

• | The receiver from the J 41397 Lower Control Arm Bushings Remover/Installer

• | J 21474-18 Nut

4. Tighten the J 21474-18 Nut until the front bushing is removed from the control arm.
5. Disassemble the bushing removal tools.
6. Assemble the following bushing removal tools as shown:

• | J 21474-27 Bolt

• | The remover/installer from the J 41211 Front Control Arm Bushing Kit

• | The receiver from the J 41211 Front Control Arm Bushing Kit

• | J 21474-4 Control Arm Bushing Set

7. Tighten the J 21474-27 Bolt until the rear bushing is removed from the control arm.
8. Disassemble the bushing removal tools.

### Installation Procedure

1. Insert the rear bushing into the control arm.

Important: Apply J 23444 A (or equivalent high pressure lubricant) to the threads of the J 21474-27 Bolt.

2. Assemble the following bushing installation tools as shown:

• | J 21474-27 Bolt

• | The receiver/installer from the J 41211 Lower Control Arm Vertical Bushing Set

• | The receiver from the J 41211 Lower Control Arm Vertical Bushing Set

• | J 21474-4 Nut

3. Tighten the J 21474-4 Nut until the rear bushing is fully seated in the control arm.
4. Disassemble the bushing installation tools.
5. Lubricate the outer casing of the front bushing.
6. Insert the front bushing into the control arm.
7. Assemble the following bushing installation tools as shown:

• | J 21474-19 Bolt

• | The remover/installer from the J 41397 Lower Control Arm Bushings

• | The receiver from the J 41397 Lower Control Arm Bushings

• | J 21474-18 Nut

8. Tighten the J 21474-19 Bolt until the front bushing is fully seated in the control arm.
9. Disassemble the bushing installation tools.
10. Install the lower control arm. Refer to Lower Control Arm Replacement.