Air Inlet Grille Panel Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Remove the windshield wiper arm assemblies. Refer to Wiper Arm Replacement in Wipers Washer Systems.
2. Remove the screws (1) from the air inlet grille (3).
3. Remove the retainers (2) from the air inlet grille (3).
4. Remove the air inlet grille (3) from the vehicle.

### Installation Procedure

1. Install the air inlet grille (3) to the vehicle.
2. Install the retainers (2) to the air inlet grille (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the screws (1) to the air inlet grille (3).

Tighten
Tighten the screws to 2 N·m (18 lb in).

4. Install the windshield wiper arm assemblies. Refer to Wiper Arm Replacement in Wipers Washer Systems.