Rear Side Door Window Regulator Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

## Rear Side Door Window Regulator Replacement Manual Windows

### Removal Procedure

1. Remove the door trim panel. Refer to Door Trim Panel Replacement .
2. Remove the water deflector in order to access the window regulator. Refer to Door Water Deflector Replacement .
3. Remove the window assembly. Refer to Window Replacement - Door.
4. Remove the power window regulator rivets (3).
5. Remove the power window regulator (1).

### Installation Procedure

1. Install the power window regulator (1).
2. Install the power window regulator rivets (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the power window regulator nuts (2).

Tighten
Tighten the nuts (2) to 10 N·m (89 lb in).

4. Install the window assembly. Refer to Window Replacement - Door.
5. Install the water deflector. Refer to Door Water Deflector Replacement .
6. Install the door trim panel. Refer to Door Trim Panel Replacement .

## Rear Side Door Window Regulator Replacement Power Windows

### Removal Procedure

1. Remove the door trim panel. Refer to Door Trim Panel Replacement .
2. Remove the water deflector in order to access the window regulator. Refer to Door Water Deflector Replacement .
3. Remove the window assembly. Refer to Window Replacement - Door.
4. Remove the manual window regulator rivets (3).
5. Remove the manual window regulator (1).

### Installation Procedure

1. Install the manual window regulator (1).
2. Install the manual window regulator rivets (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the manual window regulator nuts (2).

Tighten
Tighten the nuts (2) to 10 N·m (89 lb in).

4. Install the window assembly. Refer to Window Replacement - Door.
5. Install the water deflector. Refer to Door Water Deflector Replacement .
6. Install the door trim panel. Refer to Door Trim Panel Replacement .