Washer Pump Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Disconnect the electrical connector from the washer pump.
2. Disconnect the hose from the washer pump.
3. Remove the washer pump from the washer solvent container.

### Installation Procedure

1. Install the washer pump in the washer solvent container.

1.1. | Push the washer pump down into the washer solvent container completely.

1.2. | Push the top of the washer pump into the side of the washer solvent container.

2. Connect the hose to the washer pump.
3. Connect the electrical connector to the washer pump.