Transmitter Battery Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

Perform the following steps in order to open the transmitter case:

1. Insert a small flat-bladded tool between the 2 halves of the transmitter case at the slot provided near the key ring hole.
2. Twist the tool in order to open the case.
3. Remove the battery.

### Installation Procedure

1. Install the battery with the positive (+) side facing down.
2. Ensure the transmitter case seal is in the proper position.
3. Align the 2 halves of the transmitter case.
4. Snap the 2 halves of the transmitter case together.

Important: Normal battery life is approximately 2 years. Replace the batteries when the range of the transmitter begins to decrease significantly to less than approximately 3 m (23 ft).

5. Test the operation of the transmitter.