Steering Shaft, Lower Bearing, and Jacket - Disassemble - Off Vehicle. Chevrolet PJJ 2001

For 1990-2009 cars

1. Remove the steering column jacket. Refer to Steering Column Jacket - Disassemble - Off Vehicle .
2. Remove the lower spring retainer (5) and discard.
3. Remove the lower bearing spring (4).
4. Remove the lower bearing seat (3).
5. Remove the adapter and bearing assembly (2) from steering column jacket assembly (1).
6. Remove the steering column shaft assembly (2) from the steering column housing assembly (1).
7. Remove the 4 support screws and discard.
8. Remove the steering column support assembly from the steering column jacket assembly.