Door Lock Cylinder Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Raise the window to the full UP position.
2. Remove the door trim panel. Refer to Trim Panel Replacement - Door.
3. Remove the water deflector in order to access the lock cylinder. Refer to Water Deflector Replacement - Door.
4. Remove the lower window channel retainer. Refer to Window Channel Replacement - Door.
5. Remove the lock cylinder retaining clip (1).
6. Remove the lock rod from the lock cylinder (3).
7. Remove the lock cylinder (3).

### Installation Procedure

1. Install the lock rod to the door lock cylinder (3).
2. Install the lock cylinder (3).
3. Install the lock cylinder retaining clip (1).
4. Install the lower window channel retainer. Refer to Window Channel Replacement - Door.
5. Install the water deflector. Refer to Water Deflector Replacement - Door.
6. Install the door trim panel. Refer to Trim Panel Replacement - Door.